|  |
| --- |
| Operator Name: Date: |
| **Demonstrate the following procedures whilst disconnected from the power**

|  |  |
| --- | --- |
| Raise and lower wheeled stand |  |
| Inspect top door for tracking |  |
| Inspect bottom door for cleanliness |  |
| Check integrity of blade |  |
| Check blade tension |  |
| Set guard the correct distance from the top of the workpiece. |  |

**Demonstrate the following procedures whilst connected to power**

|  |  |
| --- | --- |
| Listen for sound of bent/broken teeth |  |
| Make straight cut |  |
| Make curved cut on appropriate bandsaw |  |

**Understand the following things**

|  |  |
| --- | --- |
| How to report faults (users should not fix problems themselves) |  |
| Meaning of no lone working rule |  |
| Blade needs to be at full speed before introduction of material |  |
| How to select mitre or rip guard |  |
| Which PPE is required or recommended (goggles required, breathing and hearing protection recommended; gloves not to be worn) |  |
| Hands should be 15cm from the blade during operation |  |
| Push sticks are required when closer than 15cm |  |
| Use of vee block when cutting round items |  |
| Need to disconnect power whilst inspecting the blade |  |
| Users must not enter yellow box areas when another user is using a power tool in that area |  |
| Users must inform other hackspace users if they are cutting anything with higher than average respiratory risks |  |
| Dust extraction must be used where available |  |
| Machine is used for wood only or some plastics |  |
| User is responsible for cleaning up |  |

 |

When competence has been achieved, tick the appropriate requirement.